8.Write an assembly language program for dividing two 16-bit datausing 8086 processor.

lhld 2100

lda 2102

mov b,a

mvi c,08

back: dad h

mov a,h

sub b

jc next

mov h,a

inr l

next: dcr c

jnz back

shld 2103

hlt