Ex no 1: write an assembly language code for addintion of two 8 bit numbers

lda 8000

mov h,a

lda 8001

add h

sta 8002

hlt