3.Write an assembly language program for adding two 16-bit datausing 8086 processor.

lhld 8000

xchg

lhld 8002

dad d

shld 8008

hlt